Name: Date:

**1)** Approximately how many Americans die each year in aerial lift accidents?

A. 10

B. 30

C. 60

D. 80

**2)** Choose all that apply. Which of the following are some of your responsibilities as an operator?

A. Complete proper training.

B. Read and understand the operator manuals.

C. Adhere to guidelines, practices for safe use, and manufacturer recommendations.

**3)** For each individual type of lift, operators must be separately qualified and authorized.

A. True

B. False

**4)** Choose all that apply. It is best practice to use fall protection for \_\_\_\_\_\_\_.

A. Articulating boom lifts

B. Elevated work platforms

C. Extensible boom platforms

D. Scissor lifts

E. Trailer-mounted aerial lifts

F. Vehicle-mounted aerial lifts

**5)** Elevated work platforms may be moved while the platform is elevated.

A. True

B. False

**6)** Choose all that apply. Which of the following is a factor for selecting the proper lift?

A. Lifting capacity

B. Worksite dimensions

C. The personal protective equipment (PPE) required

D. The lift’s power source

**7)** For lifts with multiple control panels, test each function on each panel.

A. True

B. False

**8)** Choose all that apply. Which of the following hazards should you look for during a hazard assessment?

A. Flat terrain

B. Muddy, soft terrain

C. Exposed electrical wires

D. Barriers to keep pedestrians out

**9)** Choose all that apply. What practices should you follow when moving a lift?

A. Drive slowly.

B. Raise the platform for stability.

C. Be aware of platform orientation.

D. Always face the direction of travel.

**10)** Keep the same safe distance away from 35,000 volt and 45,000 volt power lines.

A. True

B. False

**11)** Outriggers do not have to be properly set before use if the manufacturer’s recommendations indicate that the lift can be used safely without them.

A. True

B. False

**12)** Only connect your harness to anchor points outside the platform.

A. True

B. False

**Answer Key**

1. B

2. A, B & C

3. A

4. A, B, C, D, E & F

5. B

6. A, B & D

7. A

8. B & C

9. A, C & D

10. A

11. A

12. B